###############################################################################
# BRLTTY - A background process providing access to the console screen (when in
#          text mode) for a blind person using a refreshable braille display.
#
# Copyright (C) 1995-2015 by The BRLTTY Developers.
#
# BRLTTY comes with ABSOLUTELY NO WARRANTY.
#
# This is free software, placed under the terms of the
# GNU Lesser General Public License, as published by the Free Software
# Foundation; either version 2.1 of the License, or (at your option) any
# later version. Please see the file LICENSE-LGPL for details.
#
# Web Page: http://brltty.com/
#
# This software is maintained by Dave Mielke <dave@mielke.cc>.
###############################################################################

title Hedo MobilLine

note The keys behind the text cells are named routing keys.
note The rectangular navigation keys are named K1 through K3.
note The square navigation keys are named B1 through B6.
note From left to right, the navigation keys are: B3 B2 B1 K1 K2 K3 B4 B5 B6

bind K2+K1 HELP
bind K2+K3 LEARN

bind K1+K3 PREFMENU
bind K1+K3+B1 PREFLOAD
bind K1+K3+B4 PREFSAVE

bind K2 HOME
bind K1 FWINLT
bind K3 FWINRT

bind B3 TOP
bind B6 BOT

bind B2 LNUP
bind B5 LNDN

bind B1 PRDIFLN
bind B4 NXDIFLN

bind B1+B3 ATTRUP
bind B4+B6 ATTRDN

bind B1+B2 PRPGRPH
bind B4+B5 NXPGRPH

bind B2+B3 PRPROMPT
bind B5+B6 NXPROMPT

bind B1+B2+B3 PRSEARCH
bind B4+B5+B6 NXSEARCH

bind B1+K1 CHRLT
bind B1+K3 CHRRT

bind B2+K1 FWINLTSKIP
bind B2+K3 FWINRTSKIP

bind B3+K1 LNBEG
bind B3+K3 LNEND

bind B4+K1 PASTE
bind B4+K3 CSRJMP_VERT

bind B5+K1 TIME
bind B5+K3 INFO

bind B6+K1 CLIP_RESTORE
bind B6+K3 CLIP_SAVE

assign toggleOff K1
assign toggleOn K3

assign toggleKeys B1+K2
assign toggleCommand SIXDOTS
include ../toggle.kti

assign toggleKeys B2+K2
assign toggleCommand CSRTRK
include ../toggle.kti

assign toggleKeys B3+K2
assign toggleCommand DISPMD
include ../toggle.kti

assign toggleKeys B4+K2
assign toggleCommand FREEZE
include ../toggle.kti

assign toggleKeys B5+K2
assign toggleCommand CSRVIS
include ../toggle.kti

assign toggleKeys B6+K2
assign toggleCommand ATTRVIS
include ../toggle.kti

bind RoutingKey ROUTE

bind B3+RoutingKey CLIP_NEW
bind B2+RoutingKey CLIP_ADD
bind B5+RoutingKey COPY_RECT
bind B6+RoutingKey COPY_LINE

bind B1+RoutingKey PRINDENT
bind B4+RoutingKey NXINDENT

bind K1+RoutingKey SETLEFT
bind K2+RoutingKey DESCCHAR

