###############################################################################
# BRLTTY - A background process providing access to the console screen (when in
#          text mode) for a blind person using a refreshable braille display.
#
# Copyright (C) 1995-2015 by The BRLTTY Developers.
#
# BRLTTY comes with ABSOLUTELY NO WARRANTY.
#
# This is free software, placed under the terms of the
# GNU Lesser General Public License, as published by the Free Software
# Foundation; either version 2.1 of the License, or (at your option) any
# later version. Please see the file LICENSE-LGPL for details.
#
# Web Page: http://brltty.com/
#
# This software is maintained by Dave Mielke <dave@mielke.cc>.
###############################################################################

# This key subtable is for Baum displays which have 7 display keys.
note The display keys are at both ends of the text cell area, just above it.
note * The two at the left are named Display1 and Display2.
note * The large key at the right is named Display5.
note * The two immediately to its left are named Display3 and Display4.
note * The two immediately to its right are named Display6 and Display7.

bind Display5 RETURN
bind Display3 LNUP
bind Display4 LNDN
bind Display6 FWINLT
bind Display7 FWINRT

bind Display1 TOP_LEFT
bind Display2 BOT_LEFT

bind Display5+Display3 PRDIFLN
bind Display5+Display4 NXDIFLN
bind Display5+Display6 ATTRUP
bind Display5+Display7 ATTRDN

bind Display2+Display5 FREEZE
bind Display2+Display3 PRPROMPT
bind Display2+Display4 NXPROMPT
bind Display2+Display6 PRPGRPH
bind Display2+Display7 NXPGRPH

bind Display1+Display5 CSRTRK
bind Display1+Display3 DISPMD
bind Display1+Display4 SIXDOTS
bind Display1+Display6 ATTRVIS
bind Display1+Display7 CSRVIS

bind Display1+Display2+Display5 AUTOSPEAK
bind Display1+Display2+Display3 MUTE
bind Display1+Display2+Display4 SAY_LINE
bind Display1+Display2+Display6 SAY_ABOVE
bind Display1+Display2+Display7 SAY_BELOW

bind Display1+Display2 HELP
bind Display3+Display4 LEARN
bind Display6+Display7 PREFMENU
bind Display3+Display6 PREFLOAD
bind Display4+Display7 PREFSAVE

bind Display5+Display3+Display6 CSRJMP_VERT
bind Display5+Display4+Display7 PASTE

